ITEM #: ICE CREAM PASTEURIZER  
Quantity: One (1)  
Manufacturer: Carpigiani  
Model No.: Pastomaster 60 RTX   
Pertinent Data: Self Contained  
Utilities Req’d: 208V/3PH, 25.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide with 60.566 Liter every two (2) hours output.  
3. Provide 60.566 Liter Tank capacity.  
4. Provide a refrigerated extraction spigot for maximum hygiene.  
5. Provide an exchange pump for low homogenization.  
6. Provide sixteen (16) exclusive programs.  
7. Coordinate installation next to Item #, Ice Cream Maker.  
8. Provide five-year compressor warranty and two-year service/labor warranty.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.