ITEM #: ICE CUBER DISPENSER  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: DB-200H  
Pertinent Data: 200 Pounds Capacity  
Utilities Req’d: 120V/1PH; 1.4A; 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Install Item #\_\_\_\_\_\_, Ice Machine on top of Ice Dispenser, coordinate proper installation.  
4. Coordinate opening in top of bin with Item #\_\_\_\_\_\_, Ice Machine.  
5. Unit shall be all stainless steel with 6" stainless steel legs.  
6. Provide all trims required for proper installation.  
7. Provide push-button single auger agitator dispenses ice at 13 pounds per minute.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.