ITEM #: ICE DISPENSER  
Quantity: Ten (10)  
Manufacturer: Scotsman  
Model No.: HD22B-1  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 15.0A; 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Install Item #\_\_\_\_\_, Ice Maker on top of Ice Dispenser, coordinate proper installation.  
4. Coordinate opening in top of bin with Item #\_\_\_\_\_, Ice Maker.   
5. Unit shall be all stainless steel with 6" stainless steel legs.  
6. Provide all trims required for proper installation.  
7. Provide push chute to dispense ice.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.