ITEM #: ICE FLAKER WITH BIN   
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: AFE424A-1  
Pertinent Data: Self Contained Air Cooled  
Utilities Req’d: 120V/1PH; 15.0A; 3/8" CW; (2) 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide flaked ice prodction in a self contained storage bin.  
4. Provide 395 pound capacity.  
5. Provide front air flow.  
6. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
7. Provide unit with Vari-Smart Ice Level Control.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.