ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: FM-600AKE-R452-SB  
Pertinent Data: 1,323 Pounds Capacity  
Utilities Req’d: 120V/1PH; \_\_\_\_\_\_A; 3/8" CW, 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_, Ice Bin, and coordinate proper installation.  
5. Ice maker shall flake ice.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.