ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: IM-240DNE-HC-32  
Pertinent Data: 385 Pounds Capacity, Air Cooled, Stacked  
Utilities Req’d: 120V/1PH, \_\_\_\_\_A; 5/8" CW, 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Provide the connection between ice machine and Item #\_\_\_\_, Water Filtration System.  
4. Install ice machine on top of Item #\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice machine shall produce extra large cubes 1-1/4" x 1-1/4" x 1-1/4".  
6. Provide unit with an installation kit.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_, Ice Bin, flawlessly.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.