ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: IM-240DNE-HC  
Pertinent Data: 463 Pounds/210KG, Air Cooled, Cube Ice  
Utilities Req’d: 220V/1PH/50HZ, 0.9kW; 20mm CW, 20mm IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Provide the connection between ice machine and Item #\_\_\_, Water Filtration System.  
4. Install ice machine on top of Item #\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Ice machine shall produce extra large cubes 32mm x 32mm x 32mm (1-1/4" x 1-1/4" x 1-1/4").  
6. Provide unit with an installation kit.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_, Ice Bin, flawlessly.  
8. Must meet all applicable governmental, and local laws, rules, regulations, and codes.