ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: IM-50BAA-Q  
Pertinent Data: 50 Pounds Capacity, Air Cooled  
Utilities Req’d: 120V/1PH, 3.0A; 3/8" CW, 3/4" IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_, Water Filtration System.  
4. Install ice maker with self-contained Ice Bin.  
5. Ice maker shall produce 1.8" diameter sphere ice.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.