ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: KM-1900SWJ3  
Pertinent Data: 1,875 AHRI Capacity, Water Cooled  
Utilities Req’d:

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Provide the connection between ice machine and Item #\_\_\_, Water Filtration System.  
4. Install ice machine on top of Item #\_\_, Ice Bin, coordinate proper installation.  
5. Ice maker shall produce full cubes1-1/8” x 1/2” x 1-1/2” thick.  
6. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_, Ice Bin flawlessly.  
7. Must meet all applicable governmental, and local laws, rules, regulations, and codes.