ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: C0530MW-1  
Pertinent Data: 410 Pounds ARI Capacity, Water Cooled  
Utilities Req’d: 120V/1PH,13.5A; 3/8" CW, 3/4" IW; 3/8" Chilled Water Supply,   
 3/8" Chilled Water Return   
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_, Soda / Ice Dispenser, coordinate proper installation.  
5. Ice maker shall produce medium cube ice 7/8A x 7/8" x 7/8".  
6. Provide unit with KPAS which includes KVS Vari-Smart Ice Level Control, and KSBU-N Smart-Board Advance Control with Network.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_, Soda / Ice Dispenser flawlessly.