8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.  
  
ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: C0530SW-1  
Pertinent Data: 410 Pounds ARI Capacity, Water Cooled  
Utilities Req’d: 120V/1PH, 17.5A; 3/8" CW, 3/4" IW; 3/8" Chilled Water Supply (at no more than 20-80 psi, 3/8" Chilled Water Return

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice machine and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice machine on top of Item #\_\_\_\_\_\_, Ice Bin, coordinate proper installation.  
5. Provide unit with Vari-Smart Ice Level Control.  
6. Ice machine shall produce medium cubes 7/8" by 7/8" by 7/8" thick.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.