5. Ice maker shall produce nugget ice.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.  
  
ITEM #: ICE MACHINE  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: NH0922A-32  
Pertinent Data: 740 Pounds ARI Capacity, Air Cooled  
Utilities Req’d: 208V/1PH, 12.0A; 3/8” CW, 3/4” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_, Soda and Ice Dispenser, coordinate proper installation.  
5. Ice maker shall produce hard nuggets ice 3/4” x 5/16” x 3/8”.  
6. Provide unit with KPAS which includes KVS VariSmart Ice Level Control, and KSBUN SmartBoard Advance Control with Network.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_, Soda and Ice Dispenser flawlessly.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.