ITEM # : ICE MACHINE  
Quantity: One (1)  
Manufacturer: Scotsman  
Model No.: NS1322A-32  
Pertinent Data: 1300Lb., Air-Cooled, Nugget Ice  
Utilities Req’d: 208V/1PH; 17.8A; 3/8" CW; 3/4" IW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be all stainless steel construction.  
3. Coordinate with Plumbing Contractor on the connection between ice maker and Item #\_\_\_\_\_, Water Filtration System.  
4. Install ice maker on top of Item #\_\_\_\_\_, Ice Bin. Coordinate proper installation.  
5. Ice maker shall produce softer, nugget style, Original Chewable Ice.  
6. Provide unit with AutoAlert™ indicating lights, front facing removable air filter, one-touch cleaning, stainless steel finish, and AgION™ antimicrobial protection.  
7. Provide ice machine with all necessary accessories to fit onto Item #\_\_\_\_\_, Ice Bin flawlessly.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.