ITEM #: ICE TRANSPORT CART   
Quantity: One (1)  
Manufacturer: Hoshizaki  
Model No.: ITS Totes  
Pertinent Data: 175 Pound Capacity  
Utilities Req’d: —

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide all poly carts are designed for shuttle bins.  
4. Provide center split hinged lids open to the cart sides.  
5. Provide foot operated rear drain.  
6. Provide handles on both ends of cart.  
7. Provide easily maneuvered (5” front and 10” rear castors.  
8. Provide ability to slide under Item #\_\_\_\_\_\_, Ice Bin without obstruction.  
9. Must meet all applicable governmental, and local laws, rules, regulations, and codes.