ITEM #: ICE TRANSPORT CART   
Quantity: One (1)  
Manufacturer: Manitowoc  
Model No.: K-00418  
Pertinent Data: 108 KG (240 lb) Capacity  
Utilities Req’d: —

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide all poly carts are designed for shuttle bins.  
4. Provide center split hinged lids open to the cart sides.  
5. Provide foot operated rear drain.  
6. Provide six (6) (K-00416) Ice Totes to fit in the unit.  
7. Provide easily maneuvered 127mm (5”) front and 254mm (10”) rear castors.  
8. Must meet all applicable governmental, and local laws, rules, regulations, and codes.