ITEM #: INSECT CONTROL  
Quantity: One (1)  
Manufacturer: InsectOCutor  
Model No.: 1894EDGA  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 8.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide top hinged safety guard swings open; has soft gasket seal and Dual Lock fasteners for closure.  
4. Provide internal metal insect collection drawer has an extra high front baffle to prevent insect escape and particle fallout.  
5. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.