ITEM #: KNIFE SANITIZER  
Quantity: One (1)  
Manufacturer: Edlund  
Model No.: KSUV18  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 5.0A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 15-minute belled timer.  
4. Provide ability to hold up to 12 knives plus steel.  
5. Provide all stainless steel construction.  
6. Provide LED lights indicate when door is closed and sterilization is in process.  
7. Provide UV filtered plexiglass door with lockable keyed handle.  
8. Provide 2 larger slots to accommodate cleavers.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.