ITEM # KNOCK BOX  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS10.16  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.  
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication  
2. Size and configuration as shown on drawings.  
3. Provide 6” square stainless steel chute.  
4. Provide a 3/4” Diameter Hard Rubber bar attached to each side.  
5. Coordinate installation into Item #, Beverage Counter with Sink as shown on drawings.  
6. Provide shop drawings for approval prior to fabrication.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.