ITEM # : LIQUOR DISPLAY  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TS12LS  
Pertinent Data: ---  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall be placed between Item #\_\_\_\_\_\_, Soda Gun Holder, and Item #\_\_\_\_\_, Bottle Cooler.   
3. Provide a five tier display step unit, with bottle guards on each step.  
4. Unit shall have stainless steel legs with removable stainless steel shrouding to limit access under the unit.   
5. Provide shop drawings for approval prior to fabrication.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.