ITEM #: MEAL TRAY DELIVERY CART  
Quantity: One (1)  
Manufacturer: Dinex   
Model No.: DXIPICT10  
Pertinent Data: ---  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide carts which are fabricated with 1” square tubing frame with welded 18-gauge pre-formed side panels/tray slides.  
4. Provide top, bottom and single panel door shall be 18-gauge, stainless steel.   
5. Provide corner bumpers.   
6. Provide Door which has recessed door pull with a transport latch. The door has a 270° door swing with magnets to keep the door in an opened position.  
7. Provide four 5@ heavy-duty, non-marking casters, 2 swivel with brakes and 2 fixed.  
8. Provide a three (3) sided 2.35" high top rail.  
9. Provide a push handle.  
10. Equip unit with a drain assembly.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.