ITEM #: MEAL TRAY DELIVERY CART  
Quantity: One (1)  
Manufacturer: Dinex  
Model No.: DXPICTPT16  
Pertinent Data: ---  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 54" high pass-thru, one-door, one-compartment cart.  
4. Cart to have 16-tray capacity, designed to hold multiple tray sizes: 14" x 18", 15" x 20", and Dinex room service trays.  
5. Provide fixed tray slides with 5-1/4" spacing, two trays per slide.  
6. Provide corner bumpers.   
7. Unit to have 1" 18-gauge tubular frame with welded 18-gauge pre-formed side panels/tray slides.   
8. Top, bottom and single panel door to be of 18-gauge, stainless steel.   
9. Door to have recessed door pull with a top-mounted, heavy-duty drop-door latch.   
10. Provide door with 270° swing with magnets to keep the door in an opened position.  
11. Provide a push handle.  
12. Provide four 5" heavy-duty, non-marking casters, 2 swivel with brakes and 2 fixed.  
13. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.