ITEM #: MEAT GRINDER  
Quantity: One (1)  
Manufacturer: Hobart  
Model No.: 4812  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH, 7.0A  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Coordinate installation on Item #, Cold Preparation Table with Sink.  
3. Provide with heavy-duty cord and plug. Coordinate NEMA configuration with Electrical Contractor.  
4. Unit to be provided with Pull/Push On/Off Switch.  
5. Provide unit with stainless steel housing.  
6. Provide unit with spiral fluted chopping end.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.