ITEM #: MILK COOLER  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: TMC-34-S-DS-HC  
Pertinent Data: Double sided   
Utilities Req'd: 120V/1PH: 2.7A, ½” IW

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Stainless steel exterior. Stainless floor interior.  
4. Three year parts and labor warranty. Seven year compressor warranty.  
5. Provide corner bumpers.  
6. 4” casters are standard.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.