ITEM #: MIXER UTENSILTREE  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #36.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. All stainless steel construction.  
5. Flanged foot welded to 3/16" x 8" diameter stainless steel base.  
6. Provide holes in base plate for mounting to the floor.  
7. Provide 5/8" OD stainless steel tubing upright welded to flanged foot.  
8. Provide 3/8" stainless steel rods, welded to upright.  
9. Provide shop drawings for approval prior to fabrication.  
10. All finished edges shall be #7 mirrored polish finish.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.