ITEM #: MODULAR CHARCOAL OVEN  
Quantity: One (1)  
Manufacturer: Josper Basque  
Model No.: HJA-50  
Pertinent Data: Solid fuel  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Equip unit with regulation of oxygen entry.  
4. Provide chute for homogeneous distribution of oxygen.  
5. Equip unit with a charcoal combustion chamber and combustion shield.  
6. Unit shall be equipped with multiple positions for grill racks.  
7. Provide smoke exit regulation with anti-spark safety and a cooled flue.  
8. Equip unit with hydraulic door retention, thermal insulation, and upper tempering area.  
9. Unit shall be equipped with an ash drawer.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.