ITEM #: MOP SINK CABINET  
Quantity: One (1)  
Manufacturer: Advance Tabco  
Model No.: 9-OPC-84-300  
Pertinent Data: ---  
Utilities Req’d: 1/2” CW, 1/2” HW, 2” DW  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide heavy-gauge type 300 stainless steel construction.  
4. Provide 16” x 20” x 12” deep heavy-gauge type 304 stainless steel mop sink.  
5. Provide a K240 service faucet, spray hose, and spray hose bracket.  
6. Provide louvers along the top of each side panel for ventilation.  
7. Provide a sloped top for ease of cleaning.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.