ITEM #: MUG FROSTER  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: FR24-STK-TR  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 5.8A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Mug froster shall be self-contained refrigeration.  
3. Provide unit with single access door with door lock in lid.   
4. Provide unit with stainless steel interior and exterior.  
5. Provide unit with adjustable wire shelves.  
6. Unit shall be provided with heavy duty cord and plug, coordinate NEMA configuration with electrical contractor.  
7. Provide four (4) heavy duty casters, two (2) with locks.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.  
  
  
  
ITEM #: NAPKIN DISPENSER (NOT IN CONTRACT)  
Quantity: One (1)  
Pertinent Data: By Vendor