ITEM #448: OVERSHELF WITH UTENSIL RACK  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FS?.?, Detail #?.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Coordinate installation over Item #, Work Table with Bain Marie.  
5. Provide 2" x 3/16" stainless steel bar welded with stainless steel movable pot hooks at 8" on center.  
6. Provide 16-gauge stainless steel overshelf with stainless steel brackets.  
7. Ensure supports of overshelf are secured to the frame of the table for additional stability.   
8. Provide shop drawings for approval prior to fabrication.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.