Pertinent Data: ---  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Coordinate installation of P.O.S. System.  
4. Provide all stainless steel construction.  
5. Provide vented door with integral handle, and lock.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.  
  
ITEM #: P.O.S. CABINET  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TSF24POS  
Pertinent Data: ---  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Coordinate installation of Item #, P.O.S. System.  
4. Provide all stainless steel construction.  
5. Provide louvered door with integral handle.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.