ITEM #: PASS-THRU DISH DROP WINDOW  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans and Drawings #FS  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #47.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide unit with stainless steel jambs and header.  
5. Provide opening to be 30” long x 12” tall.  
6. Provide a stainless steel drop shelf, fully enclosed, extended from Item #f46, Soiled Dish Table.  
7. Provide shop drawings for approval prior to fabrication.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.