ITEM #: PASS-THRU REFRIGERATOR  
Quantity: One (1)  
Manufacturer: True Food Service Equipment   
Model No.: STA2RPT-4HS-2S-HC  
Pertinent Data: Double Section, Self-Contained  
Utilities Req’d: 120V/1PH; 5.9A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide stainless steel door, front and sides on the exterior, and aluminum sides, wall and back on the interior.  
3. Provide four (4) 6” heavy-duty swivel casters two (2) with brakes.  
4. Provide heavy-duty cord and plug.  
5. Provide two (2) full height solid doors on one side and four (4) half height solid doors on the other side, hinged as shown on plans.  
6. Provide four (4) additional wire shelves.  
7. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.