ITEM #: PASS-THRU WINDOW WITH SHELF  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans Drawing #FS  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #83  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Provide a serving shelf in a stainless steel framed window.  
5. Coordinate installation into General Contractor provided Wall Openings as shown on Drawing FS.  
6. Coordinate Fabrication and Installation with Item #, Cold Preparation Table with Sink, and Item #, Double Wall Shelf.  
7. Provide shop drawings for approval prior to fabrication.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.