ITEM #: PIZZA / FLATBREAD OVEN  
Quantity: One (1)  
Manufacturer: Wood Stone  
Model No.: WS-BL-3030  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 2.0A; 3/4” Gas @ 55,000 BTU’s  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place as shown on drawings.  
2. Provide with all standard accessories.  
3. Provide with black granite mantle.  
4. Provide stainless steel trim strips at exposed areas between pizza oven and counters.  
5. Provide an easily adjustable 55,000 BTU wall of radiant flame located at the rear of the cooking chamber.  
6. KEC to coordinate all exterior finishes and needed trim with Interior Designer.  
7. Provide gas pressure regulator and 48” quick disconnect, flexible gas hose with restraining device.  
8. Provide doorway and service panel extensions.  
9. Provide shop drawings for approval prior to fabrication.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.