ITEM #: PRE-RINSE UNIT  
Quantity: One (1)  
Manufacturer: Fisher  
Model No.: 34460  
Pertinent Data: Splash Mount  
Utilities Req'd: 1/2" HW, 1/2" CW  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Coordinate installation onto backsplash of Item #\_\_\_\_, \_\_\_\_\_\_\_\_\_.  
3. Provide with wall bracket and wrist blade handles.  
4. Provide a 12" Swing Spout.  
5. Provide back flow preventor.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.