ITEM #: PULPER PUMP  
Quantity: One (1)  
Manufacturer: Somat  
Model No.: Part Of #908  
Pertinent Data: ---  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide unite with a 3 HP pump to send and receive slurry from Item #, Pulper Extractor.  
4. Unit shall be an integral part of Item #, Pulper System.  
5. Provide shop drawings for approval prior to fabrication.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.