ITEM #213: RAPID COOK OVEN  
Quantity: One (1)  
Manufacturer: Merrychef  
Model No.: E3  
Pertinent Data: ---  
Utilities Req'd: 208V/1PH; 30.0A   
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Coordinate installation on top of Item #\_\_\_\_\_\_\_\_\_\_\_.  
4. Provide stainless steel cavity and casework.  
5. Provide (2) rack positions.  
6. Provide ventless cooking capability and EasyTouch controls.  
7. Provide USB memory and built-in diagnostic testing.  
8. Provide bottom-hinged door.  
9. Provide microwave combination mode.  
10. Equip unit with:  
a. (2) cast turntables, NSF, "40H0347ANO".  
b. (1) cool down pan "32Z4043".  
c. (1) cleaner kit "32Z4148".  
d. (1) turntable disk "40H0249".  
e. (1) oven tray handle "SR313".  
f. (1) teflon sheet "40H0190".  
g. (2) chromium plated steel racks "DR0056".  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.