ITEM #: RAPID COOK OVEN  
Quantity: One (1)  
Manufacturer: Turbo Chef  
Model No.: i3  
Pertinent Data: ---  
Utilities Req’d: 208V/1PH, 40.0A

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide 201 stainless steel interior.  
3. Provide integral recirculating catalytic converter.  
4. Provide independent bottom temperature offset  
5. Provide heavy-duty cord and plug, coordinate NEMA configuration with Electrical Contractor.  
6. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.