ITEM #: REACH-IN DOORS  
Quantity: One (1)  
Manufacturer: Anthony  
Model No.: Infinity 60 Series  
Pertinent Data: ---  
Utilities Req’d: 120V/1PH; 20.0A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide 2 pane Non-heated low E glass with Argon Gas.  
4. Equip unit with aluminum door rails.  
5. Provide Vista Arch Handle.  
6. Unit shall be equipped with Optimax Radiant OP55 LED lights.  
7. Equip unit with long lasting frame compression gasket.  
8. Provide a door stop feature which limits the door opening to 87˚ minimizing impact with adjacent door.  
9. Provide an automatic hold open.  
10. Coordinate installation into Item #???.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.