ITEM #: RECYCLING BIN  
Quantity: One (1)  
Manufacturer: Rubbermaid  
Model No.: FG9W2700BLUE  
Pertinent Data: Blue Color  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Unit shall have 50-gallon capacity.  
3. Provide heavy-duty wheels with high-performance treads are optimized for use indoors and outdoors.  
4. Equip unit with reinforced rim for superior structural integrity and robust lid designed for added strength.  
5. Units rollout lids open fully and stay in place to prevent swinging during transport.  
6. Unit shall be compliant with ANSI Standard Z245.60 (Types B and G) for compatibility with auto-lifters.  
7. Provide smooth contours and seamless construction make cleaning easier and quicker, to improve staff productivity.  
8. Unit shall be designed with an ergonomic handle for comfortable push or pull operation.  
9. Provide high-quality materials plus a UV inhibitor to extend the life of the container.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.