ITEM #: REFRIGERATED EQUIPMENT STAND  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: TRCB-72  
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 9.9A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide unit with four (4) heavy duty 16 gauge top and 20 gauge drawers.  
4. Provide each drawer fitted with Lifetime guaranteed heavy duty all metal working spec handle.  
5. Provide heavy-duty stainless steel drawer slides and rollers.  
6. Provide stainless steel front, top and sides.  
7. Provide digital temperature guage.  
8. Provide six (6) 4", heavy duty, non-marking casters, front three (3) with brakes.  
9. Coordinate installation of Item #\_\_\_\_\_\_, Modular Charbroiler, and Item #\_\_\_\_\_\_\_\_, Modular Griddle.  
10. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.