ITEM #: REFRIGERATED GRAB N GO CASE  
Quantity: One (1)  
Manufacturer: Structural Concepts  
Model No.: CO4324R-CH  
Pertinent Data: Self-Contained  
Utilities Req'd: 120V/1PH; 12.0A   
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer's standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide Breeze-E (Type II) with Energy Wise self contained refrigeration with rear access.  
4. Provide Powder coated SCC Standard Silversan Black interior, 909-58 Black laminate exterior, two (2) stainless steel mirror interior end panels, and black toe kick panel.  
5. Provide casters with levelers.  
6. Provide a 6-foot straight blade power cord.  
7. Coordinate installation into Item #\_\_\_\_\_.  
8. Provide digital Fahrenheit thermometer.  
9. Provide removable solid security cover with a lock.  
10. Provide condensate pan.  
11. Provide LED top light.  
12. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.