ITEM #: REFRIGERATED GRAB-N-GO CASE  
Quantity: One (1)  
Manufacturer: Structural Concepts  
Model No.: B3632  
Pertinent Data: Self-Contained Refrigeration  
Utilities Req’d: 120V/1PH; 16.0A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide unit with black interior, laminate standard color 909-58 black exterior, black lower front panel, and black painted exterior back panel.  
4. Provide full end panels with mirror interior.  
5. Provide four (4) non-lighted shelves.  
6. Provide top light, LED 4000K w/ frosted lens, standard.  
7. Provide digital fahrenheit thermometer.  
8. Provide six foot power cord with base exit.  
9. Provide Breeze~E (Type-ll) with EnergyWise self contained refrigeration.  
10. Provide unit with casters.  
11. Provide unit with clean sweep coil cleaner.  
12. Provide a retractable non-locking night curtain.  
13. Provide price tag moulding.  
14. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.