ITEM #: REFRIGERATED GRAB-N-GO  
Quantity: One (1)  
Manufacturer: Structural Concepts  
Model No.: HMO5136   
Pertinent Data: Self-Contained  
Utilities Req’d: 120V/1PH; 16.0A; 3/4” IW

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide a laminate exterior color. Verify with the Architect and or Interior Designer which color, pattern and grain they desire.  
4. Provide the unit with stainless steel interior.  
5. Equip the unit with a rear exterior color painted black.  
6. Provide with silver trim color.  
7. Provide unit with casters.  
8. Equip unit with a 6’ locking power cord.  
9. Provide Clean Sweep7 coil cleaner.  
10. Provide a locking, removable wire security cover.  
11. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.