ITEM #: REFRIGERATED PREP TABLE  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: TSSU-27-08D-2-HC  
Pertinent Data: Self Contained  
Utilities Req’d: 120V/1PH; 3.5A  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide self-contained refrigeration system.  
3. Provide two (2) stainless steel exterior refrigerator drawers with 250 lb drawer extension tracks.  
4. Provide recessed handles on drawers.  
5. Provide 11-3/4" deep x 1/2" thick NSF approved white polyethylene cutting board.  
6. Provide 8 pan capacity refrigerated rail with pan dividers.  
7. Provide stainless steel foam insulated flat lid.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.