ITEM #: REFRIGERATED PREP TABLE  
Quantity: One (1)  
Manufacturer: True Food Service Equipment  
Model No.: TSSU-48-12D-4-ADA-HC  
Pertinent Data: Self Contained  
Utilities Req’d: 120V/ 1PH, 5.8A

See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Provide self-contained refrigeration system.  
3. Provide four (4) stainless steel exterior refrigerator drawers with 250 lb drawer extension tracks.  
4. Provide recessed handles on drawers.  
5. Provide 11-3/4" deep x 1/2" thick NSF approved white polyethylene cutting board.  
6. Provide 12 pan capacity refrigerated rail with pan dividers.  
7. Provide stainless steel foam insulated flat lid.  
8. Coordinate installation into Item #\_\_\_\_\_\_, as shown on drawings.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.