ITEM #: SALAMANDER  
Quantity: One (1)  
Manufacturer: Jade  
Model No.: JSB-36WM   
Pertinent Data: ---  
Utilities Req’d: 3/4” Gas @ 35,000 BTU’s; 5” WC  
  
See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide counter balance mechanism.  
4. Equip unit with four locking cook positions.  
5. Provide wall mounting bracket.  
6. Coordinate installation above Item #, Six Burner Range.  
7. Provide a 3/4” gas pressure regulator.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.