ITEM #: SECURITY KNIFE CABINET  
Quantity: One (1)  
Manufacturer: IMC/Teddy  
Model No.: OC-SEC-1 (or2)-Recessed  
Pertinent Data: ---  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide top which is flat from the back to the front.  
4. Provide 18-gauge stainless steel cabinet.  
5. Provide 14-gauge stainless steel double pan full height doors.  
6. Provide two point locks with handles engage in top header and bottom shelf.  
7. Provide a knife hooks and remove shelves.  
8. Provide heavy-duty 3" welded hinges with 1/4" pins.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.