ITEM #: SLICER CART  
Quantity: One (1)  
Manufacturer: Custom Fabrication  
Model No.: Stainless Steel  
Pertinent Data: See Plans, Drawing #FS  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.   
Fabricate and set in place per plans, details, and the following:  
1. Standard fabrication Drawing #FSX.X, Detail #1A, #4C, #5A, and #14A.  
2. Set in place in location as shown on drawings.  
3. Size and configuration as shown on drawings.  
4. Unit shall be equipped 16 gauge 304 stainless steel under shelf and intermediate shelf.  
5. Provide four (4) 6” heavy duty, non-marking casters, front two (2) with brakes.  
6. Provide space on the table for Item #, Food Slicer.  
7. Fabricate and install per NSF Standard 2, complete drawings, schedules, elevations, and details.  
8. Provide shop drawings for approval prior to fabrication.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.