ITEM # : SODA GUN HOLDER  
Quantity: One (1)  
Manufacturer: Perlick  
Model No.: TSF6SGB  
Pertinent Data: For Soda Gun  
Utilities Req’d: ---  
  
See plans for location and placement of item with reference to adjoining equipment.  
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide all stainless steel construction.  
4. Provide top Cover and Manifold Mounting Bracket for both Wunder- Bar7 and Schroeder AmericaJ are included on 6@ long fillers.  
5. Provide manifold mounts to side panel for easy access and service.  
6. Provide drip cup/cradle mounts to cover.  
7. Connect to Item #\_\_\_\_\_\_.  
8. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.