ITEM #: SPREADER CABINET  
Quantity: One (1)  
Manufacturer: Imperial  
Model No.: IHR12SP  
Pertinent Data: ---  
Utilities Req’d: ---

See plans for location and placement of item with reference to adjoining equipment.   
Furnish and set in place per manufacturer’s standard specifications and the following:  
1. Set in place in location as shown on drawings.  
2. Size and configuration as shown on drawings.  
3. Provide cabinet base has a bottom shelf for storing pans and stock pots.  
4. Equip unit with a stainless steel single door.  
5. Provide cutouts in top for ingredient containers.  
6. Provide stainless steel front, sides, landing ledge and cabinet base.  
7. Unit shall have welded and polished stainless steel seams.  
8. Provide unit with four (4) 6” heavy-duty, non-marking casters, front two (2) with brakes.  
9. Must meet all applicable federal, state, and local laws, rules, regulations, and codes.